--------------------------------------------------------
EM4482 Firmware
--------------------------------------------------------
Version: 1.1.0.38
Date/Datum: 28-8-2008

English instructions, see below.

---------------
Instructies:
---------------
Let op! Voer de firmware update niet uit via een draadloze netwerk/internet verbinding.

1. Pak deze bestanden uit op je bureaublad
2. Open de Internet Explorer en ga naar het Ip-adres van de camera, bijvoorbeeld http://192.168.1.45
3. Klik op 'Setup' en log in met gebruikersnaam 'admin' en het wachtwoord '123456', tenzij dit anders ingesteld is.
4. Klik op 'Maintenance' in het menu 'Advanced'.
5. Klik op de knop 'Bladeren' en selecteer het bestand 'firmware-eng.bin'.
6. Klik op de knop 'Upgrade' waarna de firmware ingeladen wordt.
7. Wacht totdat de update voltooid is, dit kan zeker 5 minuten duren. Schakel de camera NIET uit tijdens deze procedure.
8. De camera zal automatisch opnieuw opstarten na de firmware update.
9. Ga naar 'Setup', als de camera opnieuw opgestart is.
10. Klik op 'Maintenance' in het menu 'Advanced'.
11. Klik op de knop 'Restore Default Settings'.
12. Wacht totdat de camera opnieuw opgestart is. Op het display kun je het huidige IP-adres weergegeven.
13. Schakel de camera eventueel uit door voeding van de camera te halen en opnieuw op de camera weer aan te sluiten.

De camera kan nu weer gebruikt worden.

---------------
English Instructions
---------------
Do not perform these instructions using a wireless network or internet connection.

1. Unzip the files to your desktop.
2. Open the Internet Explorer and go to the IP-address of your camera. For example: http://192.168.1.45
3. Click Setup and log in using 'admin' as a username and '123456' as a password, unless you have changed this in the past.
4. Click 'Maintentance' in the 'Advanced' menu. 
5. Click on the 'Browse' button and select the file 'firmware-eng.bin'.
6. Click on the 'Upgrade button to start the upgrade.
7. Wait until the update is complete. This can take up to 5 minutes. Do not turn off the camera during this process.
8. The camera will reboot automatically after the upgrade.
9. Go to the Setup page when the camera has been rebooted.
10. Click 'Maintentance' in the 'Advanced' menu.
11. Click on 'Restore Default Settings'.
12. Wait until the camera has been rebooted. You will see the current IP-address on the display of the camera.
13. Disconnect the power cable and plug it back in to physically reboot the camera.

The camera can be used again.

---------------
Changelog:
---------------
28-8-2008 1.1.0.38
- LED Control fixes. You can now turn off led and they will not turn on automatically again. Reboot the camera after changing this setting.
- Server Push page fixed for mobile usage.

14-8-2008 1.1.0.37
- Pan/Tilt control fixed in normal/mirror/flip/rotate modes.
- Camera will now adjust the pan/tilt controls depending on the
  selected mode under 'Basic - Image Settings'.

11-03-2008 1.1.0.36
- LED Control fixes. You can now turn off led and they will not turn on automatically again.
 
25-1-2008 1.1.0.31
- Password-less video added. try view320.html or view640.html to view video w/o password.
  Note: Guest password may not be changed for this to work.

09-1-2008 Original release
- Mail issue fixed
- Web style updated
- Typographic errors fixed