[Luz] Flash Yongnuo Speedlite YN460

Features Specifications

NG: 33

Circuit design: IGBT

Up/down ward angle: 0-90 degree

Left/right angle: 0-270 degree

Power Source: 4 X AA size batteries (Alkaline or Ni-MH are usable)

Battery Life: 100 - 1500 times (with alkaline batteries)

Recycle Time: 5 sec(with alkaline batteries)

Color Temperature: 5600K

Flash Duration: 1/800S - 1/20000S

Flash adjustment: “7 difference flash power level ( 1/1, 1/2, 1/4, 1/8, 1/16, 1/32, 1/64 )”

Power Saving: “ Stand by mode, 30mins to power off mode. 60mins to power off when using the optic mode. ”

Dimensions: 72X135X85mm

Weight: 250g

Slave mode S1: Normal optical slave

Slave mode S2: Pre-flash cancel slave